# Configuring Video Walls

Navigation: Working with Nx Witness > Video Wall Management > # Configuring Video Walls |

Initial Video Wall configuration is performed in several steps:

•Configuring Video Wall

•Configuring Layout of Video Wall Displays

•Configuring Video Wall on Several Computers

•Switching to Video Wall Mode

•Deleting Video Wall and its Elements.

Since a single computer has a limited number of available video outputs, it can a handle limited number of displays. To extend Video Wall it is necessary to add additional computers and combine them to Video Wall Cluster. See "Configuring Video Wall on Several Computers".

To change configuration refer to the following sections.