# Setting Up Camera Orientation

Navigation: Working with Nx Witness > Device Management (Cameras, Encoders and I/O Modules) > Setting Up Cameras and Devices > # Setting Up Camera Orientation |

Nx Witness can adjust to proper orientation for devices that have been mounted upside down or rotated by 90 degrees.

Note: This correction will require transcoding if exporting videos from a camera.

To specify device o rientation

1.Open Camera Settings and go to the General tab.

2.In the Image Control section, click on Auto in the Rotation field to open the pulldown menu.

3.Select the desired rotation adjustment from the available options: 0 degrees, 90 degrees, 180 degrees, 270 degrees. Select Auto to restore the original orientation.

4.Click on Apply or OK to save the setting.